|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Specification No:** | | | CTC100 / CTC150 | | | | | |
| **Tool Name:** | | | Concrete testing cube / mould. | | | | | |
| **Specification:** | | | | | | | | |
| Available in both 100mm and 150mm internal width across flats.  Manufactured from high quality cast steel. 4-part clamped for ease of extraction. Surface ground and pre greased to ensure that all surfaces are free from rust and ready to use.  Weight: 7300g & 9800g  http://www.speedcrete.co.uk/images/cube.jpg | | | | | | | | |
|  | Length (mm) | Weight | | Colour | | RCL Part No | |  |
|  | 100mm A/F | 7.8kgs | | BLUE /natural | | CTC100 | |  |
|  | 150mm A/F | 9.8kgs | | BLUE /natural | | CTC150 | |  |
|  |  |  | |  | |  | |  |
|  | | | | | | | | |
| **Status** | | | | | **Authority** | | **Date Issued** | |
| Issue 1 | | | | | W Green | | 07.04.2016 | |
| **Remarks/Notes:** | | | | | | | | |
| This product is not tested to BS requirements. | | | | | | | | |