|  |  |
| --- | --- |
| **Specification No:** | CTC100 / CTC150 |
| **Tool Name:** | Concrete testing cube / mould. |
| **Specification:**  |
| Available in both 100mm and 150mm internal width across flats.Manufactured from high quality cast steel. 4-part clamped for ease of extraction. Surface ground and pre greased to ensure that all surfaces are free from rust and ready to use. Weight: 7300g & 9800ghttp://www.speedcrete.co.uk/images/cube.jpg |
|  | Length (mm) | Weight | Colour | RCL Part No |  |
|  | 100mm A/F | 7.8kgs | BLUE /natural | CTC100 |  |
|  | 150mm A/F | 9.8kgs | BLUE /natural | CTC150 |  |
|  |  |  |  |  |  |
|   |
| **Status** | **Authority** | **Date Issued** |
| Issue 1 | W Green | 07.04.2016 |
| **Remarks/Notes:** |
| This product is not tested to BS requirements. |